**PC Blanca**

**IP – Adresses –** IP: 192.10.8.1/24, Network: 192.10.8.0, Interface: Internet

**PC Negra**

**IP – Adresses –** IP: 192.10.8.2/24, Network: 192.10.8.0, Interface: Internet

**Red Lan de los 2 Servidores**

**IP – Adresses –** IP: 20.20.20.254/24, Network: 20.20.20.0, Interface: Red\_Lan

**IP – DNS –** IP: 8.8.8.8, Allow for Remote Request

**IP – DNS – Static** **–** Name: DNS01 Address: 8.8.8.8 TTL: 1d 00:00:00

**IP – Routes –** Gateway: 192.10.8.254, Check Gateway: Ping

**IP – DHCP Server – DHCP –** DHCP Setup – DHCP Server Interface: Red\_Lan, DHCP Address Space: 20.20.20.0./24, Gateway for DHCP Network: 20.20.20.254, Address to Give Out: 20.20.20.1-20.20.20.253, DNS Servers: 8.8.8.8, Lease Time: 00:05:00

**IP – Firewall – NAT –** Chain: srnat, Src. Address: 20.20.20.0/24, Out Interface: Internet, Action: Masquerade.